                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


https://www.thingiverse.com/thing:2221310
Minimal Raspberry Pi Zero Case/Holder by Pyromaniac is licensed under the Creative Commons - Attribution - Non-Commercial license.
http://creativecommons.org/licenses/by-nc/3.0/

# Summary

I wanted to create a simple to print, detach and mount case/holder for the Raspberry Pi ZERO (W).

Load
Slice
Print
Enjoy

1. It has only one part
2. You don't need any screws
3. You have detach helper (see pictures), use a small screwdriver or something similar
4. Because of the "springs" in the middle, the case is flexible (that's why you can push the raspberry easy into it)
5. The mounting holes have a distance of 70mm, so you can also mount it on a VESA 70 Monitor/TV

(Mind the notes in "Print settings"!)

Have fun


# Print Settings

Printer: RepRap NEO
Rafts: No
Supports: No
Resolution: Z:0.1mm, Nozzle: 0.2mm
Infill: 20% Rectilinear

Notes: 
In case its to narrow for your RaspiZero, try "Slic3r"-Settings:
"Advanced" -> "Other" -> "XY Size Compensation" = "-0.15mm" (this is for my 0.2mm Nozzle, the bigger the nozzle, the higher this setting should be; and note the MINUS in the value)

See the last picture in the gallery...