                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


https://www.thingiverse.com/thing:2414631
GoPro Floaty by astroaaron is licensed under the Creative Commons - Attribution - Non-Commercial - Share Alike license.
http://creativecommons.org/licenses/by-nc-sa/3.0/

# Summary

This is a floating handle for GoPro cameras. It's only 115mm tall so it will fit on almost any printer. I have only tested it with the Hero 5, but I'm confident it will float with any other GoPro camera. For reference, the Hero 5 with the frame and a battery installed weighs ~170g.

You'll need an M5 nut for the screw and a bit string or rope <4mm in diameter for a lanyard if you want (I used paracord and it works pretty well).

# Print Settings

Printer: MP Select Mini
Rafts: No
Supports: No
Resolution: 0.2mm
Infill: 15%

Notes: 
If possible in your slicer, set the infill for everything above 98mm to 100% while keeping everything below 98mm at 15% infill. This will make the mount much sturdier while still maintaining buoyancy.