                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:3453115
Raspberry Pi 1B+...3B+ case by PETGore is licensed under the Creative Commons - Attribution license.
http://creativecommons.org/licenses/by/3.0/

# Summary

Because Raspberry Pi cases are important things in life!

Why this one sucks less than most others:
- Reduced material demand
- good venting
- durable case without any screws what so ever
- all ports open accessible
- GPIOs easily accessible due to low profile
- Large cutout for SD (not visible on photos! check the model). The bloody RPi foundation removed the spring loaded mechanism for SD release in version 3 so.

Designed to be printed with PLA at 0.15mm layer height. No supports needed, the overhangs should print fine.

The clamping gap between the lid and the bottom is currently 0.14mm which works perfectly for me. If it's too tight or too lose for you, just play with with the flow/extrusion rate. 3%-5% change should already make a difference.

Fusion 360 file included! A rugged industrial design for hat rail mount is in the making!

Post your makes ;)

# Print Settings

Printer Brand: Creality
Printer: Ender 3
Rafts: No
Supports: No
Resolution: 0.15mm layer height
Infill: 100%
Filament_brand: M4P
Filament_material: PLA

Notes: 
Flip the lid 180° in the slicer to have the bed oriented surface visible later.