                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:3460395
Inverted XTander Clip for 8BitDo SN30Pro by JezPez is licensed under the Creative Commons - Attribution license.
http://creativecommons.org/licenses/by/3.0/

# Summary

A phone clip Inverter for the 8Bitdo Xtander clip 
This clip comes in many configurations fitting: SN30 Pro, SF30 Pro, NES30 Pro, FC30 Pro, SFC30, SNES30

8BitDo made possibly the best bluetooth controller for emulation of retro games with the SN and SF30 Pro. A company Gwowo designed the 8BitDo Xstander clip holder which positions a phone vertically above the controller at an angle.

However this clip is too top heavy as the phone is heavier than the controller. To prevent the unit tipping forward, you are always gripping the controller uncomfortably tightly.

So I designed the Xtander Inverter, which repositions the phone clip part to be on-top of the controller instead of above it at an angle. This position restores the center of balance to the center of the controller (before, the center of balance was at the phone, ~2 inches above the controller). Having the center of balance at the index knuckle is ideal for long play.

You may think that it now tips backwards towards the player, but because of the thumbs being almost inside the unit now, the weight is overall better distributed and so it is comfortable at any angle.

Here is a link to the public Tinkercad model with all the steps inside (if you want the model for the joining parts, go there)
https://www.tinkercad.com/things/gIpTsL3UdSF-8bitdo-xtender-inverter-for-sn30pro

The Xtander clip for sale: 
[ebay](https://www.ebay.com.au/itm/253376490366)
[amazon](https://www.amazon.com/dp/B07B2V1SZZ/ref=cm_sw_em_r_mt_dp_U_3fiECbSFGM354)
Original clip designers: [gwowo](http://www.gwowo.com/)

PS: This is my first Thingiverse submission, thank you to this amazing community!


# Print Settings

Printer Brand: Wanhao
Printer: Wanhao Duplicator i3 Plus
Rafts: Doesn't Matter
Supports: Yes
Resolution: 0.2mm
Infill: 100%

Notes: 
Print slow ~60mm/s as this piece needs to fit with the existing Xtander bracket parts and must match their tolerances.

Actually printed on the Cocoon Create which is a rebrand of the Wanhao Duplicator i3 Plus.