                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:3483656
 by JasperPotts is licensed under the Creative Commons - Attribution - Share Alike license.
http://creativecommons.org/licenses/by-sa/3.0/

# Summary

A simple ball head for a tripod version 2. It works with medium sized camera nicely now, much more clamping force than v1.

Also I switched all the hardware over to US imperial hardware so easy to get for people doing a build in the US. You need 4 screws:

*  1/4-20 1.5" Hex Head
*  1/4-20 1" Hex Head
*  1/4-20 1" Button Head
*  6-32 1" Hex Cap Head

For the tripod mount I am using a screw in thread adaptor as a kind of metal thread insert, it came free with the gorilla pod.



# Print Settings

Printer Brand: Ultimaker
Printer: S5
Rafts: No
Supports: No
Resolution: 0.15
Infill: 40%
Filament_brand: Ultimaker
Filament_color: Black
Filament_material: Tough PLA

Notes: 
I printed all parts in one go, took 12 hours over night. After printing I had to clean a couple of the threads with a tap, 2 of the 1/4-20 and the 6-32 one. You might have been able to force it carefully but it was easier to clean as I had the correct size taps.