                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:1091071
Han Solo in Carbonite - Raspberry Pi 2/B+ Case by rigelbot is licensed under the Creative Commons - Attribution license.
http://creativecommons.org/licenses/by/3.0/

# Summary

Frozen in Carbonite by Darth Vader, Han Solo has been traded half-way across the galaxy to ultimately serve you as a budget microcomputer!

My love of Star Wars brought me to remix these two excellent models into this stellar Raspberry Pi 2/B+ case! Many thanks to Geoffro & aurelius for the original models.

Here's a time-lapse that includes my printing technique for this: https://www.youtube.com/watch?v=pwiPxT9yCPo

Enjoy!

Bleep bloop,

Rigelbot

# Print Settings

Rafts: Doesn't Matter
Supports: Yes
Resolution: Split: 0.200 for the case, 0.050 for Han Solo
Infill: 30% Fast-Honeycomb

Notes: 
Printer: Makergear M2
Slicer: Simplify3D
Filament: Hatchbox Silver PLA 1.75mm

<b>Settings:</b>
Hotend: 210°C
Heated Bed: 70°C
Split: 200 microns for the case, 50 microns for Han Solo
Adhesion: gluestick on glass + thin layer of hairspray

<b>Technique:</b>
At the 30 second mark (in the video), I had the GCODE pause with this:

G28 X0; home x-axis
M0; pause

Then I flipped the upper section on top of the lower section for the extruder to print Han Solo; effectively avoiding using supports. This saved about an hour of printing and nearly half the material weight.