                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:3651544
Nintendo Switch Console Hanger by Stetofire is licensed under the Creative Commons - Attribution license.
http://creativecommons.org/licenses/by/3.0/

# Summary

This is an accessory that allows a player to suspend the screen above them if they want to lay down and still play.
It includes four "rings" that can be used as anchor points for string.

Slide the rails on first, then connect the bottom pieces in place with the little key.

**Post Makes!**

# Print Settings

Printer Brand: Creality
Printer: Ender 3
Rafts: No
Supports: Yes
Resolution: 0.2mm
Infill: 20%
Filament_brand: Generic
Filament_material: PLA

Notes: 
**No Supports - ALMOST!**

Most of the print is designed to work supportless, but the keys need to be held up, so use your slicer to add supports to the two hook overhangs only.

If you want to print individual parts, make sure they're oriented correctly and mirrored, if needed.