                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


https://www.thingiverse.com/thing:1229473
Raspberry Pi Display Case by ftobler is licensed under the Creative Commons - Attribution license.
http://creativecommons.org/licenses/by/3.0/

# Summary

A simple display case for the Raspberry Pi 2 & 3 Model B. I used a 3.5inch touchscreen LCD, which is purchased from ebay. Link and guide is listed below. 

The micro SD card is accessible from outside. A special feature is, that it is held in place, even when the spring loaded mechanism of the sd slot fails (which happened here).

The raspi is entirely passive cooled. I have not used a heat sink or a fan.

Do not print assembly.stl. I have three different top parts. I only used and printed that width the display. I used some weak glue to bind the parts together.

<br>
#####In case you need some changes to the model to fit your Display, there is a [customizer][1]
If this is not enough for you, feel free to send me a message :)






User-specified models:
raspiBplusCase_top_differentCutout.stl
raspiBplusCase_top_extraTall.stl
<br>


[display is from ebay][2]


[guide to bring it to life][3]

(I used the raspbian image)


[1]: https://www.thingiverse.com/thing:2395683
[2]: http://www.ebay.com/itm/111717376150?_trksid=p2057872.m2749.l2649&ssPageName=STRK%3AMEBIDX%3AIT
[3]: http://www.waveshare.com/wiki/3.5inch_RPi_LCD_%28A%29