                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


https://www.thingiverse.com/thing:2473812
Attitude Indicator for Flight Simulator by alvaroalea is licensed under the Creative Commons - Attribution - Non-Commercial - Share Alike license.
http://creativecommons.org/licenses/by-nc-sa/3.0/

# Summary

Attitude Indicator for use in panel of GA Flight Simulators.
Its need 2 servos of 9gr. like SG90, and will be conected to the PC with the flight simulator via OpenCockpits Servo Board, a Arduino or similar system.

You need several M3 allen screws, about 6 normal nuts and 1 autolock nuts, at least 2 washer, 

The only piece you need to glue is the "central" to the servo horn, once attach the servo to the "soporte" pieze, ensure that the servo is centered.

You need to rotate the pieces before print.
There is a graphic file to be print in a color printer and glued over the "central" "ovalo" and "anillo" piezes.

In a future I have plans to upgrade the bezel, so I provide it twice, you can print all at once or in two parts to be upgrade in the future.

Also the "full" part is not for print, only to check how to assambly all the parts.