                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


https://www.thingiverse.com/thing:2505243
Universal tripod phone mount by neyfrota is licensed under the Creative Commons - Attribution - Non-Commercial - Share Alike license.
http://creativecommons.org/licenses/by-nc-sa/3.0/

# Summary

Yes another tripod phone mount. I have a unorthodox clamp+ballhead setup that need a compact phone holder, so i decide design my own
 
* Design 100% printable with no bolts or screws need. 
* Simple, slim and adjustable. 
* Strong as possible (few print->stress->brake->re-design cycle)

[Public cad file at onshape](https://cad.onshape.com/documents/07430178bcef17a7a378f068).

[companion blog post](https://permissiontowrite.wordpress.com/my-first-thing-at-thingiverse/)

# Print Settings


Notes: 
Recomended print settings:
* wall thickness ~1.8mm to guarantee threads print fine
* layer height <= 1.0mm to guarantee smooth walls and less friction
* infill density >70% to guarantee strong mechanical structure
* print one piece at time to avoid retraction between pieces and get better quality
* no support need