                   .:                     :,                                          
,:::::::: ::`      :::                   :::                                          
,:::::::: ::`      :::                   :::                                          
.,,:::,,, ::`.:,   ... .. .:,     .:. ..`... ..`   ..   .:,    .. ::  .::,     .:,`   
   ,::    :::::::  ::, :::::::  `:::::::.,:: :::  ::: .::::::  ::::: ::::::  .::::::  
   ,::    :::::::: ::, :::::::: ::::::::.,:: :::  ::: :::,:::, ::::: ::::::, :::::::: 
   ,::    :::  ::: ::, :::  :::`::.  :::.,::  ::,`::`:::   ::: :::  `::,`   :::   ::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  :::::: ::::::::: ::`   :::::: ::::::::: 
   ,::    ::.  ::: ::, ::`  :::.::    ::.,::  .::::: ::::::::: ::`    ::::::::::::::: 
   ,::    ::.  ::: ::, ::`  ::: ::: `:::.,::   ::::  :::`  ,,, ::`  .::  :::.::.  ,,, 
   ,::    ::.  ::: ::, ::`  ::: ::::::::.,::   ::::   :::::::` ::`   ::::::: :::::::. 
   ,::    ::.  ::: ::, ::`  :::  :::::::`,::    ::.    :::::`  ::`   ::::::   :::::.  
                                ::,  ,::                               ``             
                                ::::::::                                              
                                 ::::::                                               
                                  `,,`


http://www.thingiverse.com/thing:3640144
Raspi_box by MCMarcel is licensed under the Creative Commons - Attribution - Non-Commercial - Share Alike license.
http://creativecommons.org/licenses/by-nc-sa/3.0/

# Summary

I created a case for Raspberry,
I needed one to put in the Raspberry and a Relais.
All Ports you can plug in without opening the case.
All you need is 2 screws M5x(5-8)mm. (Made for Cylinderhead screw)
As you you see you can go through the case with the cable and fix it with cable ties.
Dimensions:
120x100x32mm


Ich hab mir ne kleine Boxx für den Raspberry incl. Relais konstruiert und gedruckt.
Man kann den Raspberry und das Relais hineinlegen, innen die Anschlüsse fertig machen und die Box verschließen. Alle anschlüsse vom Raspberry sind soweit von außen zugänglich.
Benötigt werden 2 schrauben M5x5-8mm, angefertigt ist es für Zylinderkopfschrauben.
Es sind 2 teile zu Drucken, Deckel und Unterteil.

Maße:
120x100x32mm






# Print Settings

Printer Brand: Anycubic
Printer: All-metal Mega
Rafts: No
Supports: Yes
Resolution: 0,12
Infill: 30%
Filament_brand: d.m.
Filament_color: Black
Filament_material: PLA